**AttachDetachEvents ReflectionLog**

**(CSE2920 – Events)**

How has your program changed from planning to coding to now? Explain.

Adding attach/detach events for the red button and LED was as simple as copy pasting the attach/detach evenets for the humidity sensor.

Curiously, I noticed that the humidity sensor will attach and detach when connected/disconnected from the VINT hub. The button and LED, however, only “detach” when the mini USB type B cable is disconnected from the hub.